

Lab 7

Moudie Alhousainan


Questions:


1. What are the SSIDs of the two access points that are issuing most of the beacon frames in this trace?


* Munroe St
* Linksys\_SES\_24086
* Linksys12




1. What are the intervals of time between the transmissions of the beacon frames the linksys\_ses\_24086 access point? From the 30 Munroe St. access point? (Hint: this interval of time is contained in the beacon frame itself).








3.What (in hexadecimal notation) is the source MAC address on the beacon frame from 30 Munroe St? Recall from Figure 7.13 in the text that the source, destination, and BSS are three addresses used in an 802.11 frame.

00:16:b6:f7:1d:51

1. What (in hexadecimal notation) is the destination MAC address on the beacon frame from 30 Munroe St??

ff:ff:ff:ff:ff:ff



1. What (in hexadecimal notation) is the MAC BSS id on the beacon frame from 30 Munroe St?

MAC BSS id is the MAC address of the router 00:16:b6:f7:1d:51

